{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["ERV-Submittal"],"not_rendered":{"charts":0,"images":6,"macros":1,"external_links":1,"defined_names":139,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ERV-Submittal","index":0,"n_rows":137,"n_cols":11,"rows_kept":137,"cut":false,"hidden":false,"merged":[[6,0,6,2],[7,0,7,2],[17,3,17,5],[8,0,8,2],[18,3,18,5],[0,0,0,5],[0,7,0,12],[1,0,1,1],[1,2,1,5],[1,8,1,12],[2,0,2,1],[2,8,2,12],[4,0,4,5],[5,0,5,2],[5,3,5,5],[6,3,6,5],[7,3,7,5],[8,3,8,5],[9,0,9,2],[9,3,9,5],[10,0,10,2],[10,3,10,5],[11,0,11,2],[11,3,11,5],[32,0,32,2],[16,7,16,12],[19,0,19,2],[19,3,19,5],[17,7,32,12],[28,0,28,5],[17,0,17,2],[18,0,18,2],[20,0,20,2],[20,3,20,5],[31,0,31,2],[31,3,31,5],[21,0,21,2],[21,3,21,5],[22,0,22,2],[22,3,22,5],[23,0,23,2],[23,3,23,5],[24,0,24,2],[24,3,24,5],[131,0,131,12],[132,0,133,12],[66,0,66,12],[44,7,44,8],[32,3,32,5],[40,7,40,12],[63,0,63,5],[41,7,41,8],[44,10,44,11],[33,3,33,5],[42,7,42,8],[43,7,43,8],[35,0,35,2],[35,3,35,5],[33,0,33,2],[61,0,62,6],[62,7,62,12],[47,0,47,5],[42,10,42,11],[45,10,45,11],[35,7,35,12],[36,7,36,8],[36,10,36,11],[37,7,37,8],[37,0,37,5],[41,0,41,2],[42,0,42,2],[43,0,43,2],[44,0,44,2],[45,0,45,2],[50,7,50,8],[50,10,50,11],[42,3,42,5],[43,3,43,5],[37,10,37,11],[38,10,38,11],[44,3,44,5],[41,3,41,5],[12,0,12,2],[12,3,12,5],[13,0,13,2],[13,3,13,5],[14,0,14,2],[14,3,14,5],[16,0,16,5],[30,3,30,5],[25,0,25,2],[25,3,25,5],[26,0,26,2],[26,3,26,5],[29,3,29,5],[29,0,29,2],[30,0,30,2],[34,0,34,2],[34,3,34,5],[70,0,70,5],[136,0,142,12],[135,0,135,8],[47,7,47,8],[48,10,48,11],[48,7,48,8],[49,10,49,11],[43,10,43,11],[47,10,47,11],[41,10,41,11],[46,10,46,11],[45,7,45,8],[46,7,46,8],[49,7,49,8],[38,7,38,8],[57,0,57,1],[45,3,45,5],[58,0,58,1],[60,0,60,6],[60,7,60,12],[48,0,48,5],[61,7,61,12]]}
[null,null,null,null,null,null,null,"Indoor Standalone ERV"]
["Project Name",null,null,null,null,null,null,"Model #"]
["Quantity",null,null,null,null,null,null,"Tag #"]
[]
["SUMMER PERFORMANCE"]
["Outside Air Dry Bulb ˚F"]
["Outside Air Wet Bulb ˚F"]
["Return Air Dry Bulb ˚F"]
["Return Air Wet Bulb ˚F"]
["Supply Air Dry Bulb ˚F"]
["Supply Air Wet Bulb ˚F"]
["Total Heat Recovered (btu/h)"]
["Total Heat Recovered (tons)"]
["Sensible Effectiveness (%)"]
["Total Effectiveness (%)"]
[]
["WINTER PERFORMANCE",null,null,null,null,null,null,"STANDARD FEATURES"]
["Outside Air Dry Bulb ˚F",null,null,null,null,null,null,"• Standard 2” MERV 8 filters\n• Intergrated variable exhaust and outside air fans\n• AHRI rated Energy recovery wheel.\n• Standard double wall construction\n• Polyurathan insulation"]
["Outside Air Wet Bulb ˚F"]
["Return Air Dry Bulb ˚F"]
["Return Air Wet Bulb ˚F"]
["Supply Air Dry Bulb ˚F"]
["Supply Air Wet Bulb ˚F"]
["Total Heat Recovered (btu/h)"]
["Total Heat Recovered (tons)"]
["Sensible Effectiveness (%)"]
["Total Effectiveness (%)"]
[]
["BLOWER PERFORMANCE"]
["Supply Air (hp)"]
["Supply Air (cfm)"]
["Supply Air ESP (in-wc)"]
["Return Air (hp)"]
["Return Air (cfm)"]
["Return Air ESP (in-wc)"]
["Unit Configuration",null,null,null,null,null,null,"CONTROLS"]
[null,null,null,null,null,null,null,"Electro Mech"]
["ELECTRICAL DATA"]
["208v 1 Ph.",null,"230v 1 Ph.",null,"460v 3 Ph."]
["208v 3 Ph.",null,"230v 3 Ph."]
[null,null,null,null,null,null,null,"OPTIONAL FEATURES"]
["Supply Blower (qty / amps)",null,null,null,null,null,null,"2-Position OA Damper",null,null,"Humidity sensor"]
["Exhaust Blower (qty / amps)",null,null,null,null,null,null,"2-Position EA Damper",null,null,"Supply duct static pressure control"]
["Wheel Motor (amps)",null,null,null,null,null,null,"ultraGUARD exterior coatings",null,null,"Exhaust building pressure control"]
["MCA (amps)",null,null,null,null,null,null,"MERV 13 Filters",null,null,"Frost protection"]
["MOCP (amps)",null,null,null,null,null,null,"Filter status switch",null,null,"OA airflow monitoring & control"]
[null,null,null,null,null,null,null,"Fan status switch",null,null,"EA airflow monitoring & control"]
["UNIT WEIGHT (lbs)",null,null,null,null,null,null,"Purge wheel",null,null,"Bacnet translator"]
[null,null,null,null,null,null,null,"Sensible wheel",null,null,"365 Annual timer"]
[null,null,null,null,null,null,null,"Bypass OA damper"]
[]
[null,null,null,null,null,null,null,"Note:  Humidity & Bypass OA damper can not be joined with Electro Mech controls"]
[]
[]
[]
[]
[]
[]
[]
[]
["NOTES",null,null,null,null,null,null,"WARRANTY"]
[null,null,null,null,null,null,null,"Thrity (30) Day Labor from the day of startup or Ninty (90) Days from shipping date, which ever comes first."]
[null,null,null,null,null,null,null,"One (1) Year Limited Parts-Only Warranty on the Complete Unit."]
["PD 1/7/19 - v 1.1 | www.myiaire.com | © 2019 iAIRE, LLC"]
[]
[]
["DIMENSIONAL SUBMITTAL"]
[]
[]
[]
["DIMENSIONS"]
["A","B","C","D","E","F"]
[55,52,50,32,24,24]
[]
["G","H","CLEARANCE"]
[2.5,2.5,44]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["SEQUENCE OF OPERATIONS"]
[]
[]
[]
["ELECTRO MECHANICAL CONTROL"]
["In the UNOCCUPIED mode, the ERV unit will be off and the outside air damper, if supplied, will be closed. Occupied or Unoccupied is signaled to the IAIRE controller via an open or closed contact on the OCCUPIED input with a clock or switch. An open contact on the input indicates UNOCCUPIED, a closed contact indicates OCCUPIED.\n\nIn the OCCUPIED mode, the outside air damper will open, the supply fan will ramp up to the configured fan speed and the wheel will turn on.\n"]